1. Download the driver [Profilic\_Win8\_x64\_x86](http://ananddrs.com/wp-content/uploads/2014/09/Profilic_Win8_x64_x86.zip) and extract it

2. Open Device Manager3. Expand Ports (COM & LPT)

4. Right click device name Prolifc USB-to-Serial Comm Port and select Property

5. Select Driver tab

6. Click Update Driver

7. Choose Browse my computer for driver software

8. Choose Let me pick from a list of device drivers on my computer

9. Click Have Disk

10. Choose the folder that you extracted from the downloaded zip file.

11. Choose file "ser2pl.inf" and click Open

12. Click OK

13. After successfully installed restart your PC.

* Windows 8/8.1/10 are NOT supported in PL-2303HXA and PL-2303X [EOL](http://www.prolific.com.tw/US/ShowProduct.aspx?p_id=212&pcid=41) chip versions.
* Run PL2303 CheckChipVersion tool program in Windows XP/Vista/7 to check chip version.
* Windows XP, 2000, 98 and Windows ME driver technical support is discontinued.
* Prolific recommends to use [**PL-2303HXD (HX Rev D) or PL2303TA**](http://www.prolific.com.tw/US/supportDownload.aspx?FileType=58&FileID=133&pcid=85&Page=0) chip.